# Required Components

|  |  |
| --- | --- |
| Three 3D printed parts, labeled 1-3 from top to bottom | **BOM**   1. Slide-on Trigger Attachment 2. Shoulder Bumper Extender 3. Shoulder Trigger Extender |

# Required Tools

* Sandpaper
* Hobby knife

# Assembly Instructions

## Step 1

Slide the trigger attachment over the centre section of the Joy-Con holder

|  |
| --- |
| Nintendo Joy-Con Grip with Slide-On Trigger Attachment. Arrows show what direction it slides on from. |

## Step 2

Insert both Joy-Cons into the holder.

|  |
| --- |
| Assembly from previous step with both joycons now inserted |

## Step 3

Clip the trigger extender onto the bottom slot of the trigger attachment

|  |
| --- |
| Previous assembly flipped upside down, with the trigger extender attached to the bottom slot |

## Step 4

Attach the bumper extender to the top slot of the trigger attachment

|  |
| --- |
| Assembly right-side up, with bumper extender attached to the top slot |